{
  "design": {
    "design_info": {
      "boundary_crc": "0x5199E03713246BDA",
      "device": "xcku040-ffva1156-2-i",
      "gen_directory": "../../../../radar_alinx_kintex.gen/sources_1/bd/decimation_bd",
      "name": "decimation_bd",
      "rev_ctrl_bd_flag": "RevCtrlBdOff",
      "synth_flow_mode": "Singular",
      "tool_version": "2022.2",
      "validated": "true"
    },
    "design_tree": {
      "axis_broadcaster_0": "",
      "dec_2_width": "",
      "dec_2_fir": "",
      "dec_8_fir": "",
      "dec_4_fir": "",
      "dec_16_fir": "",
      "axis_broadcaster_1": "",
      "axis_broadcaster_2": "",
      "dec_4_width": "",
      "dec_16_width": "",
      "dec_8_width": ""
    },
    "interface_ports": {
      "dec_by_2": {
        "mode": "Master",
        "vlnv_bus_definition": "xilinx.com:interface:axis:1.0",
        "vlnv": "xilinx.com:interface:axis_rtl:1.0",
        "parameters": {
          "CLK_DOMAIN": {
            "value": "decimation_bd_clk",
            "value_src": "default"
          },
          "FREQ_HZ": {
            "value": "280000000"
          },
          "HAS_TKEEP": {
            "value": "0",
            "value_src": "default"
          },
          "HAS_TLAST": {
            "value": "0",
            "value_src": "default"
          },
          "HAS_TREADY": {
            "value": "1",
            "value_src": "default"
          },
          "HAS_TSTRB": {
            "value": "0",
            "value_src": "default"
          },
          "INSERT_VIP": {
            "value": "0",
            "value_src": "default"
          },
          "LAYERED_METADATA": {
            "value": "undef",
            "value_src": "default"
          },
          "PHASE": {
            "value": "0.0",
            "value_src": "default"
          },
          "TDATA_NUM_BYTES": {
            "value": "12",
            "value_src": "default_prop"
          },
          "TDEST_WIDTH": {
            "value": "0",
            "value_src": "default"
          },
          "TID_WIDTH": {
            "value": "0",
            "value_src": "default"
          },
          "TUSER_WIDTH": {
            "value": "0",
            "value_src": "default"
          }
        },
        "port_maps": {
          "TVALID": {
            "physical_name": "dec_by_2_tvalid",
            "direction": "O"
          },
          "TREADY": {
            "physical_name": "dec_by_2_tready",
            "direction": "I"
          },
          "TDATA": {
            "physical_name": "dec_by_2_tdata",
            "direction": "O",
            "left": "95",
            "right": "0"
          }
        }
      },
      "dec_by_4": {
        "mode": "Master",
        "vlnv_bus_definition": "xilinx.com:interface:axis:1.0",
        "vlnv": "xilinx.com:interface:axis_rtl:1.0",
        "parameters": {
          "CLK_DOMAIN": {
            "value": "decimation_bd_clk",
            "value_src": "default"
          },
          "FREQ_HZ": {
            "value": "280000000"
          },
          "HAS_TKEEP": {
            "value": "0",
            "value_src": "default"
          },
          "HAS_TLAST": {
            "value": "0",
            "value_src": "default"
          },
          "HAS_TREADY": {
            "value": "1",
            "value_src": "default"
          },
          "HAS_TSTRB": {
            "value": "0",
            "value_src": "default"
          },
          "INSERT_VIP": {
            "value": "0",
            "value_src": "default"
          },
          "LAYERED_METADATA": {
            "value": "undef",
            "value_src": "default"
          },
          "PHASE": {
            "value": "0.0",
            "value_src": "default"
          },
          "TDATA_NUM_BYTES": {
            "value": "12",
            "value_src": "default_prop"
          },
          "TDEST_WIDTH": {
            "value": "0",
            "value_src": "default"
          },
          "TID_WIDTH": {
            "value": "0",
            "value_src": "default"
          },
          "TUSER_WIDTH": {
            "value": "0",
            "value_src": "default"
          }
        },
        "port_maps": {
          "TVALID": {
            "physical_name": "dec_by_4_tvalid",
            "direction": "O"
          },
          "TREADY": {
            "physical_name": "dec_by_4_tready",
            "direction": "I"
          },
          "TDATA": {
            "physical_name": "dec_by_4_tdata",
            "direction": "O",
            "left": "95",
            "right": "0"
          }
        }
      },
      "in_i": {
        "mode": "Slave",
        "vlnv_bus_definition": "xilinx.com:interface:axis:1.0",
        "vlnv": "xilinx.com:interface:axis_rtl:1.0",
        "parameters": {
          "CLK_DOMAIN": {
            "value": "decimation_bd_clk",
            "value_src": "default"
          },
          "FREQ_HZ": {
            "value": "280000000"
          },
          "HAS_TKEEP": {
            "value": "0"
          },
          "HAS_TLAST": {
            "value": "0"
          },
          "HAS_TREADY": {
            "value": "1"
          },
          "HAS_TSTRB": {
            "value": "0"
          },
          "INSERT_VIP": {
            "value": "0",
            "value_src": "default"
          },
          "LAYERED_METADATA": {
            "value": "undef"
          },
          "PHASE": {
            "value": "0.0",
            "value_src": "default"
          },
          "TDATA_NUM_BYTES": {
            "value": "8"
          },
          "TDEST_WIDTH": {
            "value": "0"
          },
          "TID_WIDTH": {
            "value": "0"
          },
          "TUSER_WIDTH": {
            "value": "0"
          }
        },
        "port_maps": {
          "TDATA": {
            "physical_name": "in_i_tdata",
            "direction": "I",
            "left": "63",
            "right": "0"
          },
          "TREADY": {
            "physical_name": "in_i_tready",
            "direction": "O"
          },
          "TVALID": {
            "physical_name": "in_i_tvalid",
            "direction": "I"
          }
        }
      },
      "dec_by_8": {
        "mode": "Master",
        "vlnv_bus_definition": "xilinx.com:interface:axis:1.0",
        "vlnv": "xilinx.com:interface:axis_rtl:1.0",
        "parameters": {
          "CLK_DOMAIN": {
            "value": "decimation_bd_clk",
            "value_src": "default"
          },
          "FREQ_HZ": {
            "value": "280000000"
          },
          "HAS_TKEEP": {
            "value": "0",
            "value_src": "default"
          },
          "HAS_TLAST": {
            "value": "0",
            "value_src": "default"
          },
          "HAS_TREADY": {
            "value": "1",
            "value_src": "default"
          },
          "HAS_TSTRB": {
            "value": "0",
            "value_src": "default"
          },
          "INSERT_VIP": {
            "value": "0",
            "value_src": "default"
          },
          "LAYERED_METADATA": {
            "value": "undef",
            "value_src": "default"
          },
          "PHASE": {
            "value": "0.0",
            "value_src": "default"
          },
          "TDATA_NUM_BYTES": {
            "value": "12",
            "value_src": "default_prop"
          },
          "TDEST_WIDTH": {
            "value": "0",
            "value_src": "default"
          },
          "TID_WIDTH": {
            "value": "0",
            "value_src": "default"
          },
          "TUSER_WIDTH": {
            "value": "0",
            "value_src": "default"
          }
        },
        "port_maps": {
          "TVALID": {
            "physical_name": "dec_by_8_tvalid",
            "direction": "O"
          },
          "TREADY": {
            "physical_name": "dec_by_8_tready",
            "direction": "I"
          },
          "TDATA": {
            "physical_name": "dec_by_8_tdata",
            "direction": "O",
            "left": "95",
            "right": "0"
          }
        }
      },
      "dec_by_16": {
        "mode": "Master",
        "vlnv_bus_definition": "xilinx.com:interface:axis:1.0",
        "vlnv": "xilinx.com:interface:axis_rtl:1.0",
        "parameters": {
          "CLK_DOMAIN": {
            "value": "decimation_bd_clk",
            "value_src": "default"
          },
          "FREQ_HZ": {
            "value": "280000000"
          },
          "HAS_TKEEP": {
            "value": "0",
            "value_src": "default"
          },
          "HAS_TLAST": {
            "value": "0",
            "value_src": "default"
          },
          "HAS_TREADY": {
            "value": "1",
            "value_src": "default"
          },
          "HAS_TSTRB": {
            "value": "0",
            "value_src": "default"
          },
          "INSERT_VIP": {
            "value": "0",
            "value_src": "default"
          },
          "LAYERED_METADATA": {
            "value": "undef",
            "value_src": "default"
          },
          "PHASE": {
            "value": "0.0",
            "value_src": "default"
          },
          "TDATA_NUM_BYTES": {
            "value": "12",
            "value_src": "default_prop"
          },
          "TDEST_WIDTH": {
            "value": "0",
            "value_src": "default"
          },
          "TID_WIDTH": {
            "value": "0",
            "value_src": "default"
          },
          "TUSER_WIDTH": {
            "value": "0",
            "value_src": "default"
          }
        },
        "port_maps": {
          "TVALID": {
            "physical_name": "dec_by_16_tvalid",
            "direction": "O"
          },
          "TREADY": {
            "physical_name": "dec_by_16_tready",
            "direction": "I"
          },
          "TDATA": {
            "physical_name": "dec_by_16_tdata",
            "direction": "O",
            "left": "95",
            "right": "0"
          }
        }
      }
    },
    "ports": {
      "clk": {
        "type": "clk",
        "direction": "I",
        "parameters": {
          "ASSOCIATED_BUSIF": {
            "value": "dec_by_2:in_i:dec_by_4:dec_by_8:dec_by_16"
          },
          "ASSOCIATED_RESET": {
            "value": "rstn"
          },
          "CLK_DOMAIN": {
            "value": "decimation_bd_clk",
            "value_src": "default"
          },
          "FREQ_HZ": {
            "value": "280000000"
          },
          "FREQ_TOLERANCE_HZ": {
            "value": "0",
            "value_src": "default"
          },
          "INSERT_VIP": {
            "value": "0",
            "value_src": "default"
          },
          "PHASE": {
            "value": "0.0",
            "value_src": "default"
          }
        }
      },
      "rstn": {
        "type": "rst",
        "direction": "I",
        "parameters": {
          "INSERT_VIP": {
            "value": "0",
            "value_src": "default"
          },
          "POLARITY": {
            "value": "ACTIVE_LOW",
            "value_src": "default"
          }
        }
      }
    },
    "components": {
      "axis_broadcaster_0": {
        "vlnv": "xilinx.com:ip:axis_broadcaster:1.1",
        "xci_name": "decimation_bd_axis_broadcaster_0_0",
        "xci_path": "ip/decimation_bd_axis_broadcaster_0_0/decimation_bd_axis_broadcaster_0_0.xci",
        "inst_hier_path": "axis_broadcaster_0"
      },
      "dec_2_width": {
        "vlnv": "xilinx.com:ip:axis_dwidth_converter:1.1",
        "xci_name": "decimation_bd_axis_dwidth_converter_0_0",
        "xci_path": "ip/decimation_bd_axis_dwidth_converter_0_0/decimation_bd_axis_dwidth_converter_0_0.xci",
        "inst_hier_path": "dec_2_width",
        "parameters": {
          "M_TDATA_NUM_BYTES": {
            "value": "12"
          }
        }
      },
      "dec_2_fir": {
        "vlnv": "xilinx.com:ip:fir_compiler:7.2",
        "xci_name": "decimation_bd_fir_compiler_0_0",
        "xci_path": "ip/decimation_bd_fir_compiler_0_0/decimation_bd_fir_compiler_0_0.xci",
        "inst_hier_path": "dec_2_fir",
        "parameters": {
          "Clock_Frequency": {
            "value": "300.0"
          },
          "CoefficientVector": {
            "value": [
              "-1.56146976e-18, -1.88787840e-03,  2.24491365e-18,  3.86247830e-03, -4.19119720e-18, -8.24246660e-03,  7.10401637e-18,  1.59471140e-02, -1.05399209e-17, -2.86765592e-02,  1.39758253e-17, ",
              "5.07185616e-02, -1.68886445e-17, -9.80159075e-02,  1.88349281e-17,  3.15941764e-01,  5.00705787e-01,  3.15941764e-01,  1.88349281e-17, -9.80159075e-02, -1.68886445e-17,  5.07185616e-02, ",
              "1.39758253e-17, -2.86765592e-02, -1.05399209e-17,  1.59471140e-02,  7.10401637e-18, -8.24246660e-03, -4.19119720e-18,  3.86247830e-03,  2.24491365e-18, -1.88787840e-03, -1.56146976e-18"
            ]
          },
          "Coefficient_Fractional_Bits": {
            "value": "15"
          },
          "Coefficient_Sets": {
            "value": "1"
          },
          "Coefficient_Sign": {
            "value": "Signed"
          },
          "Coefficient_Structure": {
            "value": "Symmetric"
          },
          "Coefficient_Width": {
            "value": "16"
          },
          "ColumnConfig": {
            "value": "17"
          },
          "Data_Fractional_Bits": {
            "value": "15"
          },
          "Data_Width": {
            "value": "16"
          },
          "Decimation_Rate": {
            "value": "2"
          },
          "Filter_Architecture": {
            "value": "Systolic_Multiply_Accumulate"
          },
          "Filter_Type": {
            "value": "Decimation"
          },
          "Has_ARESETn": {
            "value": "true"
          },
          "Interpolation_Rate": {
            "value": "1"
          },
          "Number_Channels": {
            "value": "1"
          },
          "Output_Rounding_Mode": {
            "value": "Truncate_LSBs"
          },
          "Output_Width": {
            "value": "17"
          },
          "Quantization": {
            "value": "Quantize_Only"
          },
          "RateSpecification": {
            "value": "Input_Sample_Period"
          },
          "SamplePeriod": {
            "value": "0.25"
          },
          "Sample_Frequency": {
            "value": "0.001"
          },
          "Zero_Pack_Factor": {
            "value": "1"
          }
        }
      },
      "dec_8_fir": {
        "vlnv": "xilinx.com:ip:fir_compiler:7.2",
        "xci_name": "decimation_bd_dec_2_fir_0",
        "xci_path": "ip/decimation_bd_dec_2_fir_0/decimation_bd_dec_2_fir_0.xci",
        "inst_hier_path": "dec_8_fir",
        "parameters": {
          "Clock_Frequency": {
            "value": "300.0"
          },
          "CoefficientVector": {
            "value": [
              "-1.56146976e-18, -1.88787840e-03,  2.24491365e-18,  3.86247830e-03, -4.19119720e-18, -8.24246660e-03,  7.10401637e-18,  1.59471140e-02, -1.05399209e-17, -2.86765592e-02,  1.39758253e-17, ",
              "5.07185616e-02, -1.68886445e-17, -9.80159075e-02,  1.88349281e-17,  3.15941764e-01,  5.00705787e-01,  3.15941764e-01,  1.88349281e-17, -9.80159075e-02, -1.68886445e-17,  5.07185616e-02, ",
              "1.39758253e-17, -2.86765592e-02, -1.05399209e-17,  1.59471140e-02,  7.10401637e-18, -8.24246660e-03, -4.19119720e-18,  3.86247830e-03,  2.24491365e-18, -1.88787840e-03, -1.56146976e-18"
            ]
          },
          "Coefficient_Fractional_Bits": {
            "value": "15"
          },
          "Coefficient_Sets": {
            "value": "1"
          },
          "Coefficient_Sign": {
            "value": "Signed"
          },
          "Coefficient_Structure": {
            "value": "Symmetric"
          },
          "Coefficient_Width": {
            "value": "16"
          },
          "ColumnConfig": {
            "value": "9"
          },
          "Data_Fractional_Bits": {
            "value": "15"
          },
          "Data_Width": {
            "value": "18"
          },
          "Decimation_Rate": {
            "value": "2"
          },
          "Filter_Architecture": {
            "value": "Systolic_Multiply_Accumulate"
          },
          "Filter_Type": {
            "value": "Decimation"
          },
          "Has_ARESETn": {
            "value": "true"
          },
          "Interpolation_Rate": {
            "value": "1"
          },
          "Number_Channels": {
            "value": "1"
          },
          "Output_Rounding_Mode": {
            "value": "Truncate_LSBs"
          },
          "Output_Width": {
            "value": "19"
          },
          "Quantization": {
            "value": "Quantize_Only"
          },
          "RateSpecification": {
            "value": "Input_Sample_Period"
          },
          "SamplePeriod": {
            "value": "1"
          },
          "Sample_Frequency": {
            "value": "0.001"
          },
          "Zero_Pack_Factor": {
            "value": "1"
          }
        }
      },
      "dec_4_fir": {
        "vlnv": "xilinx.com:ip:fir_compiler:7.2",
        "xci_name": "decimation_bd_dec_2_fir_1",
        "xci_path": "ip/decimation_bd_dec_2_fir_1/decimation_bd_dec_2_fir_1.xci",
        "inst_hier_path": "dec_4_fir",
        "parameters": {
          "Clock_Frequency": {
            "value": "300.0"
          },
          "CoefficientVector": {
            "value": [
              "-1.56146976e-18, -1.88787840e-03,  2.24491365e-18,  3.86247830e-03, -4.19119720e-18, -8.24246660e-03,  7.10401637e-18,  1.59471140e-02, -1.05399209e-17, -2.86765592e-02,  1.39758253e-17, ",
              "5.07185616e-02, -1.68886445e-17, -9.80159075e-02,  1.88349281e-17,  3.15941764e-01,  5.00705787e-01,  3.15941764e-01,  1.88349281e-17, -9.80159075e-02, -1.68886445e-17,  5.07185616e-02, ",
              "1.39758253e-17, -2.86765592e-02, -1.05399209e-17,  1.59471140e-02,  7.10401637e-18, -8.24246660e-03, -4.19119720e-18,  3.86247830e-03,  2.24491365e-18, -1.88787840e-03, -1.56146976e-18"
            ]
          },
          "Coefficient_Fractional_Bits": {
            "value": "15"
          },
          "Coefficient_Sets": {
            "value": "1"
          },
          "Coefficient_Sign": {
            "value": "Signed"
          },
          "Coefficient_Structure": {
            "value": "Symmetric"
          },
          "Coefficient_Width": {
            "value": "16"
          },
          "ColumnConfig": {
            "value": "17"
          },
          "Data_Fractional_Bits": {
            "value": "15"
          },
          "Data_Width": {
            "value": "17"
          },
          "Decimation_Rate": {
            "value": "2"
          },
          "Filter_Architecture": {
            "value": "Systolic_Multiply_Accumulate"
          },
          "Filter_Type": {
            "value": "Decimation"
          },
          "Has_ARESETn": {
            "value": "true"
          },
          "Interpolation_Rate": {
            "value": "1"
          },
          "Number_Channels": {
            "value": "1"
          },
          "Output_Rounding_Mode": {
            "value": "Truncate_LSBs"
          },
          "Output_Width": {
            "value": "18"
          },
          "Quantization": {
            "value": "Quantize_Only"
          },
          "RateSpecification": {
            "value": "Input_Sample_Period"
          },
          "SamplePeriod": {
            "value": "0.5"
          },
          "Sample_Frequency": {
            "value": "0.001"
          },
          "Zero_Pack_Factor": {
            "value": "1"
          }
        }
      },
      "dec_16_fir": {
        "vlnv": "xilinx.com:ip:fir_compiler:7.2",
        "xci_name": "decimation_bd_dec_2_fir_2",
        "xci_path": "ip/decimation_bd_dec_2_fir_2/decimation_bd_dec_2_fir_2.xci",
        "inst_hier_path": "dec_16_fir",
        "parameters": {
          "Clock_Frequency": {
            "value": "300.0"
          },
          "CoefficientVector": {
            "value": [
              "-1.56146976e-18, -1.88787840e-03,  2.24491365e-18,  3.86247830e-03, -4.19119720e-18, -8.24246660e-03,  7.10401637e-18,  1.59471140e-02, -1.05399209e-17, -2.86765592e-02,  1.39758253e-17, ",
              "5.07185616e-02, -1.68886445e-17, -9.80159075e-02,  1.88349281e-17,  3.15941764e-01,  5.00705787e-01,  3.15941764e-01,  1.88349281e-17, -9.80159075e-02, -1.68886445e-17,  5.07185616e-02, ",
              "1.39758253e-17, -2.86765592e-02, -1.05399209e-17,  1.59471140e-02,  7.10401637e-18, -8.24246660e-03, -4.19119720e-18,  3.86247830e-03,  2.24491365e-18, -1.88787840e-03, -1.56146976e-18"
            ]
          },
          "Coefficient_Fractional_Bits": {
            "value": "15"
          },
          "Coefficient_Sets": {
            "value": "1"
          },
          "Coefficient_Sign": {
            "value": "Signed"
          },
          "Coefficient_Structure": {
            "value": "Symmetric"
          },
          "Coefficient_Width": {
            "value": "16"
          },
          "ColumnConfig": {
            "value": "5"
          },
          "Data_Fractional_Bits": {
            "value": "15"
          },
          "Data_Width": {
            "value": "19"
          },
          "Decimation_Rate": {
            "value": "2"
          },
          "Filter_Architecture": {
            "value": "Systolic_Multiply_Accumulate"
          },
          "Filter_Type": {
            "value": "Decimation"
          },
          "Has_ARESETn": {
            "value": "true"
          },
          "Interpolation_Rate": {
            "value": "1"
          },
          "Number_Channels": {
            "value": "1"
          },
          "Output_Rounding_Mode": {
            "value": "Truncate_LSBs"
          },
          "Output_Width": {
            "value": "20"
          },
          "Quantization": {
            "value": "Quantize_Only"
          },
          "RateSpecification": {
            "value": "Input_Sample_Period"
          },
          "SamplePeriod": {
            "value": "2"
          },
          "Sample_Frequency": {
            "value": "0.001"
          },
          "Zero_Pack_Factor": {
            "value": "1"
          }
        }
      },
      "axis_broadcaster_1": {
        "vlnv": "xilinx.com:ip:axis_broadcaster:1.1",
        "xci_name": "decimation_bd_axis_broadcaster_0_1",
        "xci_path": "ip/decimation_bd_axis_broadcaster_0_1/decimation_bd_axis_broadcaster_0_1.xci",
        "inst_hier_path": "axis_broadcaster_1"
      },
      "axis_broadcaster_2": {
        "vlnv": "xilinx.com:ip:axis_broadcaster:1.1",
        "xci_name": "decimation_bd_axis_broadcaster_0_2",
        "xci_path": "ip/decimation_bd_axis_broadcaster_0_2/decimation_bd_axis_broadcaster_0_2.xci",
        "inst_hier_path": "axis_broadcaster_2"
      },
      "dec_4_width": {
        "vlnv": "xilinx.com:ip:axis_dwidth_converter:1.1",
        "xci_name": "decimation_bd_dec_2_width_0",
        "xci_path": "ip/decimation_bd_dec_2_width_0/decimation_bd_dec_2_width_0.xci",
        "inst_hier_path": "dec_4_width",
        "parameters": {
          "M_TDATA_NUM_BYTES": {
            "value": "12"
          }
        }
      },
      "dec_16_width": {
        "vlnv": "xilinx.com:ip:axis_dwidth_converter:1.1",
        "xci_name": "decimation_bd_dec_2_width_1",
        "xci_path": "ip/decimation_bd_dec_2_width_1/decimation_bd_dec_2_width_1.xci",
        "inst_hier_path": "dec_16_width",
        "parameters": {
          "M_TDATA_NUM_BYTES": {
            "value": "12"
          }
        }
      },
      "dec_8_width": {
        "vlnv": "xilinx.com:ip:axis_dwidth_converter:1.1",
        "xci_name": "decimation_bd_dec_2_width_2",
        "xci_path": "ip/decimation_bd_dec_2_width_2/decimation_bd_dec_2_width_2.xci",
        "inst_hier_path": "dec_8_width",
        "parameters": {
          "M_TDATA_NUM_BYTES": {
            "value": "12"
          }
        }
      }
    },
    "interface_nets": {
      "axis_broadcaster_0_M00_AXIS": {
        "interface_ports": [
          "axis_broadcaster_0/M00_AXIS",
          "dec_2_width/S_AXIS"
        ]
      },
      "axis_broadcaster_0_M01_AXIS": {
        "interface_ports": [
          "axis_broadcaster_0/M01_AXIS",
          "dec_4_fir/S_AXIS_DATA"
        ]
      },
      "axis_broadcaster_1_M00_AXIS": {
        "interface_ports": [
          "axis_broadcaster_1/M00_AXIS",
          "dec_4_width/S_AXIS"
        ]
      },
      "axis_broadcaster_1_M01_AXIS": {
        "interface_ports": [
          "axis_broadcaster_1/M01_AXIS",
          "dec_8_fir/S_AXIS_DATA"
        ]
      },
      "axis_broadcaster_2_M00_AXIS": {
        "interface_ports": [
          "axis_broadcaster_2/M00_AXIS",
          "dec_8_width/S_AXIS"
        ]
      },
      "axis_broadcaster_2_M01_AXIS": {
        "interface_ports": [
          "axis_broadcaster_2/M01_AXIS",
          "dec_16_fir/S_AXIS_DATA"
        ]
      },
      "dec_16_fir_M_AXIS_DATA": {
        "interface_ports": [
          "dec_16_fir/M_AXIS_DATA",
          "dec_16_width/S_AXIS"
        ]
      },
      "dec_16_width_M_AXIS": {
        "interface_ports": [
          "dec_by_16",
          "dec_16_width/M_AXIS"
        ]
      },
      "dec_2_fir_M_AXIS_DATA": {
        "interface_ports": [
          "dec_2_fir/M_AXIS_DATA",
          "axis_broadcaster_0/S_AXIS"
        ]
      },
      "dec_2_width_M_AXIS": {
        "interface_ports": [
          "dec_by_2",
          "dec_2_width/M_AXIS"
        ]
      },
      "dec_4_fir_M_AXIS_DATA": {
        "interface_ports": [
          "dec_4_fir/M_AXIS_DATA",
          "axis_broadcaster_1/S_AXIS"
        ]
      },
      "dec_4_width_M_AXIS": {
        "interface_ports": [
          "dec_by_4",
          "dec_4_width/M_AXIS"
        ]
      },
      "dec_8_fir_M_AXIS_DATA": {
        "interface_ports": [
          "dec_8_fir/M_AXIS_DATA",
          "axis_broadcaster_2/S_AXIS"
        ]
      },
      "dec_8_width_M_AXIS": {
        "interface_ports": [
          "dec_by_8",
          "dec_8_width/M_AXIS"
        ]
      },
      "in_i_1": {
        "interface_ports": [
          "in_i",
          "dec_2_fir/S_AXIS_DATA"
        ]
      }
    },
    "nets": {
      "Net": {
        "ports": [
          "clk",
          "dec_2_fir/aclk",
          "axis_broadcaster_0/aclk",
          "dec_4_fir/aclk",
          "axis_broadcaster_1/aclk",
          "dec_8_fir/aclk",
          "axis_broadcaster_2/aclk",
          "dec_16_fir/aclk",
          "dec_2_width/aclk",
          "dec_4_width/aclk",
          "dec_16_width/aclk",
          "dec_8_width/aclk"
        ]
      },
      "Net1": {
        "ports": [
          "rstn",
          "axis_broadcaster_0/aresetn",
          "dec_2_fir/aresetn",
          "dec_4_fir/aresetn",
          "axis_broadcaster_1/aresetn",
          "dec_8_fir/aresetn",
          "axis_broadcaster_2/aresetn",
          "dec_16_fir/aresetn",
          "dec_4_width/aresetn",
          "dec_8_width/aresetn",
          "dec_2_width/aresetn",
          "dec_16_width/aresetn"
        ]
      }
    }
  }
}