<?xml version="1.0" encoding="utf-8"?>
<graphml xmlns="http://graphml.graphdrawing.org/xmlns" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://graphml.graphdrawing.org/xmlns http://graphml.graphdrawing.org/xmlns/1.0/graphml.xsd">
  <key id="BA" for="node" attr.name="base_addr" attr.type="string"/>
  <key id="BP" for="node" attr.name="base_param" attr.type="string"/>
  <key id="EH" for="edge" attr.name="edge_hid" attr.type="int"/>
  <key id="HA" for="node" attr.name="high_addr" attr.type="string"/>
  <key id="HP" for="node" attr.name="high_param" attr.type="string"/>
  <key id="LT" for="node" attr.name="lock_type" attr.type="string"/>
  <key id="MA" for="node" attr.name="master_addrspace" attr.type="string"/>
  <key id="MX" for="node" attr.name="master_instance" attr.type="string"/>
  <key id="MI" for="node" attr.name="master_interface" attr.type="string"/>
  <key id="MS" for="node" attr.name="master_segment" attr.type="string"/>
  <key id="MV" for="node" attr.name="master_vlnv" attr.type="string"/>
  <key id="TM" for="node" attr.name="memory_type" attr.type="string"/>
  <key id="SX" for="node" attr.name="slave_instance" attr.type="string"/>
  <key id="SI" for="node" attr.name="slave_interface" attr.type="string"/>
  <key id="MM" for="node" attr.name="slave_memmap" attr.type="string"/>
  <key id="SS" for="node" attr.name="slave_segment" attr.type="string"/>
  <key id="SV" for="node" attr.name="slave_vlnv" attr.type="string"/>
  <key id="TU" for="node" attr.name="usage_type" attr.type="string"/>
  <key id="VH" for="node" attr.name="vert_hid" attr.type="int"/>
  <key id="VM" for="node" attr.name="vert_name" attr.type="string"/>
  <key id="VT" for="node" attr.name="vert_type" attr.type="string"/>
  <graph id="G" edgedefault="undirected" parse.nodeids="canonical" parse.edgeids="canonical" parse.order="nodesfirst">
    <node id="n0">
      <data key="BA">0x81010000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x8101FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_axil_dma_ctrl1_Reg</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/</data>
      <data key="SI">axil_dma_ctrl1</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n1">
      <data key="BA">0x80120000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x8012FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_axil_data_gen_Reg</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/</data>
      <data key="SI">axil_data_gen</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n2">
      <data key="BA">0x40000000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x4000FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_axi_timer_0_Reg</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/axi_timer_0</data>
      <data key="SI">S_AXI</data>
      <data key="SS">Reg</data>
      <data key="SV">xilinx.com:ip:axi_timer:2.0</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n3">
      <data key="VH">2</data>
      <data key="VM">design_1</data>
      <data key="VT">VR</data>
    </node>
    <node id="n4">
      <data key="BA">0x0000000000</data>
      <data key="BP">axibar_0</data>
      <data key="HA">0xFFFFFFFFFF</data>
      <data key="HP">axibar_highaddr_0</data>
      <data key="MA">pcie_m_axi1</data>
      <data key="MX">/</data>
      <data key="MI">pcie_m_axi1</data>
      <data key="MS">SEG_xdma_0_BAR0</data>
      <data key="MV">:::</data>
      <data key="TM">both</data>
      <data key="SX">/xdma_0</data>
      <data key="SI">S_AXI_B</data>
      <data key="SS">BAR0</data>
      <data key="SV">xilinx.com:ip:xdma:4.1</data>
      <data key="TU">memory</data>
      <data key="VT">AC</data>
    </node>
    <node id="n5">
      <data key="BA">0x80000000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x8000FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_axil_descriptors_Reg</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/</data>
      <data key="SI">axil_descriptors</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n6">
      <data key="BA">0x80110000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x8011FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_axil_timing_Reg</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/</data>
      <data key="SI">axil_timing</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n7">
      <data key="BA">0x83000000</data>
      <data key="BP">baseaddr</data>
      <data key="HA">0x83FFFFFF</data>
      <data key="HP">highaddr</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_xdma_0_CTL0</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/xdma_0</data>
      <data key="SI">S_AXI_LITE</data>
      <data key="SS">CTL0</data>
      <data key="SV">xilinx.com:ip:xdma:4.1</data>
      <data key="TU">memory</data>
      <data key="VT">AC</data>
    </node>
    <node id="n8">
      <data key="BA">0x81000000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x8100FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_axil_dma_ctrl0_Reg</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/</data>
      <data key="SI">axil_dma_ctrl0</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n9">
      <data key="BA">0x0080100000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x008010FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">M_AXI_B</data>
      <data key="MX">/xdma_0</data>
      <data key="MI">M_AXI_B</data>
      <data key="MS">SEG_axil_util_Reg</data>
      <data key="MV">xilinx.com:ip:xdma:4.1</data>
      <data key="TM">both</data>
      <data key="SX">/</data>
      <data key="SI">axil_util</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n10">
      <data key="BA">0x40030000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x4003FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_system_management_wiz_0_Reg</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/system_management_wiz_0</data>
      <data key="SI">S_AXI_LITE</data>
      <data key="SS">Reg</data>
      <data key="SV">xilinx.com:ip:system_management_wiz:1.3</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n11">
      <data key="VM">design_1</data>
      <data key="VT">BC</data>
    </node>
    <node id="n12">
      <data key="BA">0x0081000000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x008100FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">M_AXI_B</data>
      <data key="MX">/xdma_0</data>
      <data key="MI">M_AXI_B</data>
      <data key="MS">SEG_axil_dma_ctrl0_Reg</data>
      <data key="MV">xilinx.com:ip:xdma:4.1</data>
      <data key="TM">both</data>
      <data key="SX">/</data>
      <data key="SI">axil_dma_ctrl0</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n13">
      <data key="BA">0x0080000000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x008000FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">M_AXI_B</data>
      <data key="MX">/xdma_0</data>
      <data key="MI">M_AXI_B</data>
      <data key="MS">SEG_axil_descriptors_Reg</data>
      <data key="MV">xilinx.com:ip:xdma:4.1</data>
      <data key="TM">both</data>
      <data key="SX">/</data>
      <data key="SI">axil_descriptors</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n14">
      <data key="BA">0x00000000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x00007FFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">DLMB</data>
      <data key="MS">SEG_dlmb_bram_if_cntlr_Mem</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/microblaze_0_local_memory/dlmb_bram_if_cntlr</data>
      <data key="SI">SLMB</data>
      <data key="SS">Mem</data>
      <data key="SV">xilinx.com:ip:lmb_bram_if_cntlr:4.0</data>
      <data key="TU">memory</data>
      <data key="VT">AC</data>
    </node>
    <node id="n15">
      <data key="TU">active</data>
      <data key="VH">2</data>
      <data key="VT">PM</data>
    </node>
    <node id="n16">
      <data key="BA">0x00000000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x00007FFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Instruction</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">ILMB</data>
      <data key="MS">SEG_ilmb_bram_if_cntlr_Mem</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">instruction</data>
      <data key="SX">/microblaze_0_local_memory/ilmb_bram_if_cntlr</data>
      <data key="SI">SLMB</data>
      <data key="SS">Mem</data>
      <data key="SV">xilinx.com:ip:lmb_bram_if_cntlr:4.0</data>
      <data key="TU">memory</data>
      <data key="VT">AC</data>
    </node>
    <node id="n17">
      <data key="BA">0x0080110000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x008011FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">M_AXI_B</data>
      <data key="MX">/xdma_0</data>
      <data key="MI">M_AXI_B</data>
      <data key="MS">SEG_axil_timing_Reg</data>
      <data key="MV">xilinx.com:ip:xdma:4.1</data>
      <data key="TM">both</data>
      <data key="SX">/</data>
      <data key="SI">axil_timing</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n18">
      <data key="BA">0x0083000000</data>
      <data key="BP">baseaddr</data>
      <data key="HA">0x0083FFFFFF</data>
      <data key="HP">highaddr</data>
      <data key="MA">M_AXI_B</data>
      <data key="MX">/xdma_0</data>
      <data key="MI">M_AXI_B</data>
      <data key="MS">SEG_xdma_0_CTL0</data>
      <data key="MV">xilinx.com:ip:xdma:4.1</data>
      <data key="TM">both</data>
      <data key="SX">/xdma_0</data>
      <data key="SI">S_AXI_LITE</data>
      <data key="SS">CTL0</data>
      <data key="SV">xilinx.com:ip:xdma:4.1</data>
      <data key="TU">memory</data>
      <data key="VT">AC</data>
    </node>
    <node id="n19">
      <data key="BA">0x0080120000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x008012FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">M_AXI_B</data>
      <data key="MX">/xdma_0</data>
      <data key="MI">M_AXI_B</data>
      <data key="MS">SEG_axil_data_gen_Reg</data>
      <data key="MV">xilinx.com:ip:xdma:4.1</data>
      <data key="TM">both</data>
      <data key="SX">/</data>
      <data key="SI">axil_data_gen</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n20">
      <data key="BA">0x0081010000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x008101FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">M_AXI_B</data>
      <data key="MX">/xdma_0</data>
      <data key="MI">M_AXI_B</data>
      <data key="MS">SEG_axil_dma_ctrl1_Reg</data>
      <data key="MV">xilinx.com:ip:xdma:4.1</data>
      <data key="TM">both</data>
      <data key="SX">/</data>
      <data key="SI">axil_dma_ctrl1</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n21">
      <data key="BA">0x80100000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x8010FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_axil_util_Reg</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/</data>
      <data key="SI">axil_util</data>
      <data key="SS">Reg</data>
      <data key="SV">::design_1_imp:</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n22">
      <data key="BA">0x40010000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x4001FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_axi_uartlite_0_Reg</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/axi_uartlite_0</data>
      <data key="SI">S_AXI</data>
      <data key="SS">Reg</data>
      <data key="SV">xilinx.com:ip:axi_uartlite:2.0</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <node id="n23">
      <data key="BA">0x0000000000</data>
      <data key="BP">axibar_0</data>
      <data key="HA">0xFFFFFFFFFF</data>
      <data key="HP">axibar_highaddr_0</data>
      <data key="MA">pcie_m_axi0</data>
      <data key="MX">/</data>
      <data key="MI">pcie_m_axi0</data>
      <data key="MS">SEG_xdma_0_BAR0</data>
      <data key="MV">:::</data>
      <data key="TM">both</data>
      <data key="SX">/xdma_0</data>
      <data key="SI">S_AXI_B</data>
      <data key="SS">BAR0</data>
      <data key="SV">xilinx.com:ip:xdma:4.1</data>
      <data key="TU">memory</data>
      <data key="VT">AC</data>
    </node>
    <node id="n24">
      <data key="BA">0x40020000</data>
      <data key="BP">C_BASEADDR</data>
      <data key="HA">0x4002FFFF</data>
      <data key="HP">C_HIGHADDR</data>
      <data key="MA">Data</data>
      <data key="MX">/microblaze_0</data>
      <data key="MI">M_AXI_DP</data>
      <data key="MS">SEG_microblaze_0_axi_intc_Reg</data>
      <data key="MV">xilinx.com:ip:microblaze:11.0</data>
      <data key="TM">data</data>
      <data key="SX">/microblaze_0_axi_intc</data>
      <data key="SI">s_axi</data>
      <data key="MM">S_AXI</data>
      <data key="SS">Reg</data>
      <data key="SV">xilinx.com:ip:axi_intc:4.1</data>
      <data key="TU">register</data>
      <data key="VT">AC</data>
    </node>
    <edge id="e0" source="n11" target="n3"/>
    <edge id="e1" source="n3" target="n15"/>
    <edge id="e2" source="n23" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e3" source="n4" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e4" source="n2" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e5" source="n22" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e6" source="n1" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e7" source="n5" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e8" source="n8" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e9" source="n0" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e10" source="n6" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e11" source="n21" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e12" source="n14" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e13" source="n24" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e14" source="n10" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e15" source="n7" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e16" source="n16" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e17" source="n19" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e18" source="n13" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e19" source="n12" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e20" source="n20" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e21" source="n17" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e22" source="n9" target="n15">
      <data key="EH">2</data>
    </edge>
    <edge id="e23" source="n18" target="n15">
      <data key="EH">2</data>
    </edge>
  </graph>
</graphml>
